 AI

AI 33
                                         Ku-band Operation Report

                                        Ku-band Operation Report

                                                                                                    Hidetaka Izumiyama

                                                                     Japan Satellite Systems Inc.

izu@jcsat.co.jp

                                       Overview

                                      Overview

u

                   We confirmed that Ku-band link can be

                   used for International Internet connectivity

                   But, sometimes we lost the connectivity.

                                       The reason of IP unreachable

                                      The reason of IP unreachable

u

                   Satellite link

                         u

                                         Rain degradation is short time(see fig HKUST)

u

                   VSAT equipment

                         u

                                         Electrial Power Down if UPS is not

                                         installed.(ITB)

                         u

                                         Un-stable Uplink Power(see fig ITB)

                                                  u

                                                              we need more study on that

                                                              the satellite is focused clearly on sight?

                                       The reason of IP

                                      The reason of IP

                                       unreachable(Cont.)

                                      unreachable(Cont.)

u

                   Gatway PC

                         u

                                         Inappropriate Riscom card with the Gateway

                                         PC(HKUST)

u

                   Operation

                         u

                                         short notice or miss annoucement for scheduled

                                         down

                         u

                                         WIDE internet re-numbering

                                         BGP-4 issue (peering , penalty)

                                       For analysis of satellite link...

                                      For analysis of satellite link...

u

                   Developed

                         u

                                         Satellite link carrier monitoring

                                         system(http://ix-jp2.ai3.net)

                         u

                                         Satellite link trafic monitoring

                                         system(http://www.ai3.net/traffic)

u

                   Request for Partner side

                         u

                                         install the tool and gather its log data for our f

                                         uture analysis

                                         how can we get weather data in your country ?

                                       Conclusion

                                      Conclusion

u

                   Ku-band rain degradation is not a major r

                   eason for IP reachable.

u

                   Ku-band rain degradation does not contiune l

                   ong time.

u

                   We should keep gathering more detailed

                   data for analysis.

                   Let´s make reseach report together.

                                       Context

                                      Context

u

                   Overview

u

                   The reason of IP unreachable

u

                   For analisis of satellite link....

                   Conclusion